NET "UC_WEB_IN" CLOCK_DEDICATED_ROUTE = FALSE;
NET "UC_REB_IN" CLOCK_DEDICATED_ROUTE = FALSE;
NET "CLKREF_TCXO" CLOCK_DEDICATED_ROUTE = FALSE;
# Added 10% timing margin for operation over extended temperature
NET "CLKREF_TCXO" TNM_NET = CLKREF_TCXO;
TIMESPEC TS_CLKREF_TCXO = PERIOD "CLKREF_TCXO" 19.2 MHz HIGH 50%;
NET "CLKREF_EXT" TNM_NET = CLKREF_EXT;
TIMESPEC TS_CLKREF_EXT = PERIOD "CLKREF_EXT" 10 MHz HIGH 50%;
NET "CLKREF_DDR3" TNM_NET = CLKREF_DDR3;
TIMESPEC TS_CLKREF_TCXO = PERIOD "CLKREF_DDR3" 100 MHz HIGH 50%;
NET "UC_REB_IN" TNM_NET = "UC_REB_IN";
TIMESPEC TS_UC_REB_IN = PERIOD "UC_REB_IN" 55 MHz HIGH 50%;
NET "UC_WEB_IN" TNM_NET = "UC_WEB_IN";
TIMESPEC TS_UC_WEB_IN = PERIOD "UC_WEB_IN" 55 MHz HIGH 50%;
NET "ASYNC_RESET" TIG = TS_CLKREF_TCXO;
NET "ASYNC_RESET_D" TIG = TS_CLKREF_TCXO;
NET "DNA_ID_001/CLK_DIV2" TNM_NET = DNA_ID_001/CLK_DIV2;
TIMESPEC TS_DNA_ID_001_CLK_DIV2 = PERIOD "DNA_ID_001/CLK_DIV2" 20 MHz HIGH 50%;

##----------------------------------------------------------------
## CLOCKs
##----------------------------------------------------------------
NET "CLKREF_TCXO" LOC = AB16;
NET "CLKREF_EXT" LOC = AB17;
NET "CLKREF_DDR3" LOC = F21;
#NET "CLKREF200_LVDS_IN[0]" LOC = AA16;
#NET "CLKREF200_LVDS_IN[1]" LOC = Y16;
#
NET "CLKREF_TCXO" IOSTANDARD = LVCMOS33;
NET "CLKREF_EXT" IOSTANDARD = LVCMOS33;
NET "CLKREF_DDR3" IOSTANDARD = LVCMOS33;
#
##----------------------------------------------------------------
## ARM MICRO
##----------------------------------------------------------------
#NET "UC_AD[0]" LOC = P22;
#NET "UC_AD[1]" LOC = R22;
#NET "UC_AD[2]" LOC = P21;
#NET "UC_AD[3]" LOC = R21;
#NET "UC_AD[4]" LOC = T21;
#NET "UC_AD[5]" LOC = U21;
#NET "UC_AD[6]" LOC = P19;
#NET "UC_AD[7]" LOC = R19;
#NET "UC_ALE_IN" LOC = V18;
#NET "UC_CSIB_IN" LOC = V17;
#NET "UC_REB_IN" LOC = AA19;
#NET "UC_WEB_IN" LOC = W17;
#
#NET "UC_AD[0]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[1]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[2]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[3]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[4]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[5]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[6]" IOSTANDARD = LVCMOS33;
#NET "UC_AD[7]" IOSTANDARD = LVCMOS33;
#NET "UC_ALE_IN" IOSTANDARD = LVCMOS33;
#NET "UC_CSIB_IN" IOSTANDARD = LVCMOS33;
#NET "UC_REB_IN" IOSTANDARD = LVCMOS33;
#NET "UC_WEB_IN" IOSTANDARD = LVCMOS33;
#
#NET "UC_ALE_IN" PULLDOWN;
#NET "UC_CSIB_IN" PULLUP;
#NET "UC_REB_IN" PULLUP;
#NET "UC_WEB_IN" PULLUP;
#
##----------------------------------------------------------------
## TEST POINTS
##----------------------------------------------------------------
#NET "TP[1]" LOC = Y13;
#NET "TP[2]" LOC = V13;
#NET "TP[3]" LOC = AB12;
#NET "TP[4]" LOC = Y12;
#NET "TP[5]" LOC = W12;
#NET "TP[6]" LOC = AB11;
#NET "TP[7]" LOC = AA11;
#NET "TP[8]" LOC = Y11;
#NET "TP[9]" LOC = W11;
#NET "TP[10]" LOC = AB10;
#NET "TP[11]" LOC = AA10;
#NET "TP[12]" LOC = AA9;
#NET "TP[13]" LOC = W10;
#NET "TP[14]" LOC = V10;
#
#NET "TP[1]" IOSTANDARD = LVCMOS33;
#NET "TP[2]" IOSTANDARD = LVCMOS33;
#NET "TP[3]" IOSTANDARD = LVCMOS33;
#NET "TP[4]" IOSTANDARD = LVCMOS33;
#NET "TP[5]" IOSTANDARD = LVCMOS33;
#NET "TP[6]" IOSTANDARD = LVCMOS33;
#NET "TP[7]" IOSTANDARD = LVCMOS33;
#NET "TP[8]" IOSTANDARD = LVCMOS33;
#NET "TP[9]" IOSTANDARD = LVCMOS33;
#NET "TP[10]" IOSTANDARD = LVCMOS33;
#NET "TP[11]" IOSTANDARD = LVCMOS33;
#NET "TP[12]" IOSTANDARD = LVCMOS33;
#NET "TP[13]" IOSTANDARD = LVCMOS33;
#NET "TP[14]" IOSTANDARD = LVCMOS33;
#
#NET "AUX_DAC_S[1]" LOC = Y17;
#NET "AUX_DAC_S[2]" LOC = W16;
#NET "AUX_DAC_S[3]" LOC = W15;
#
#NET "AUX_DAC_S[1]" IOSTANDARD = LVCMOS33; 
#NET "AUX_DAC_S[2]" IOSTANDARD = LVCMOS33; 
#NET "AUX_DAC_S[3]" IOSTANDARD = LVCMOS33; 

#----------------------------------------------------------------
# DDR3 SODIMM memory module
#----------------------------------------------------------------
# see DDR3_CONTROLLER.UCF

#----------------------------------------------------------------
# RIGHT CONNECTOR
#----------------------------------------------------------------
NET   "RIGHT_CONNECTOR_A[1]"                             LOC = "Y1";
NET   "RIGHT_CONNECTOR_A[2]"                             LOC = "W1";
NET   "RIGHT_CONNECTOR_A[3]"                             LOC = "W4";
NET   "RIGHT_CONNECTOR_A[4]"                             LOC = "V4";
NET   "RIGHT_CONNECTOR_A[5]"                             LOC = "V8";
NET   "RIGHT_CONNECTOR_A[6]"                             LOC = "V9";
NET   "RIGHT_CONNECTOR_A[7]"                             LOC = "V2";
NET   "RIGHT_CONNECTOR_A[8]"                             LOC = "U2";
NET   "RIGHT_CONNECTOR_A[9]"                             LOC = "U5";
NET   "RIGHT_CONNECTOR_A[10]"                             LOC = "T5";
NET   "RIGHT_CONNECTOR_A[11]"                             LOC = "U1";
NET   "RIGHT_CONNECTOR_A[12]"                             LOC = "T1";
NET   "RIGHT_CONNECTOR_A[13]"                             LOC = "T4";
NET   "RIGHT_CONNECTOR_A[14]"                             LOC = "R4";
NET   "RIGHT_CONNECTOR_A[15]"                             LOC = "P1";
NET   "RIGHT_CONNECTOR_A[16]"                             LOC = "R1";
NET   "RIGHT_CONNECTOR_A[17]"                             LOC = "P4";
NET   "RIGHT_CONNECTOR_A[18]"                             LOC = "P5";
NET   "RIGHT_CONNECTOR_A[19]"                             LOC = "N5";
NET   "RIGHT_CONNECTOR_A[20]"                             LOC = "P6";
NET   "RIGHT_CONNECTOR_A[21]"                             LOC = "M5";
NET   "RIGHT_CONNECTOR_A[22]"                             LOC = "M6";
NET   "RIGHT_CONNECTOR_A[23]"                             LOC = "K3";
NET   "RIGHT_CONNECTOR_A[24]"                             LOC = "L3";
NET   "RIGHT_CONNECTOR_A[25]"                             LOC = "J1";
NET   "RIGHT_CONNECTOR_A[26]"                             LOC = "K1";
NET   "RIGHT_CONNECTOR_A[27]"                             LOC = "J4";
NET   "RIGHT_CONNECTOR_A[28]"                             LOC = "K4";
NET   "RIGHT_CONNECTOR_A[29]"                             LOC = "H5";
NET   "RIGHT_CONNECTOR_A[30]"                             LOC = "J5";
NET   "RIGHT_CONNECTOR_A[31]"                             LOC = "G3";
NET   "RIGHT_CONNECTOR_A[32]"                             LOC = "H3";
NET   "RIGHT_CONNECTOR_A[33]"                             LOC = "E3";
NET   "RIGHT_CONNECTOR_A[34]"                             LOC = "F3";
NET   "RIGHT_CONNECTOR_A[35]"                             LOC = "D2";
NET   "RIGHT_CONNECTOR_A[36]"                             LOC = "E2";
NET   "RIGHT_CONNECTOR_A[37]"                             LOC = "B2";
NET   "RIGHT_CONNECTOR_A[38]"                             LOC = "C2";

NET   "RIGHT_CONNECTOR_B1[1]"                             LOC = "Y2";
NET   "RIGHT_CONNECTOR_B1[2]"                             LOC = "W2";
NET   "RIGHT_CONNECTOR_B1[3]"                             LOC = "W7";
NET   "RIGHT_CONNECTOR_B1[4]"                             LOC = "V7";
NET   "RIGHT_CONNECTOR_B2[6]"                             LOC = "V5";
NET   "RIGHT_CONNECTOR_B2[7]"                             LOC = "U6";
NET   "RIGHT_CONNECTOR_B2[8]"                             LOC = "V3";
NET   "RIGHT_CONNECTOR_B2[9]"                             LOC = "U3";
NET   "RIGHT_CONNECTOR_B2[10]"                             LOC = "R2";
NET   "RIGHT_CONNECTOR_B2[11]"                             LOC = "R3";
NET   "RIGHT_CONNECTOR_B2[12]"                             LOC = "T6";
NET   "RIGHT_CONNECTOR_B2[13]"                             LOC = "R6";
NET   "RIGHT_CONNECTOR_B2[14]"                             LOC = "N2";
NET   "RIGHT_CONNECTOR_B2[15]"                             LOC = "P2";
NET   "RIGHT_CONNECTOR_B2[16]"                             LOC = "N3";
NET   "RIGHT_CONNECTOR_B2[17]"                             LOC = "N4";
NET   "RIGHT_CONNECTOR_B2[18]"                             LOC = "M2";
NET   "RIGHT_CONNECTOR_B2[19]"                             LOC = "M3";
NET   "RIGHT_CONNECTOR_B3[21]"                             LOC = "L1";
NET   "RIGHT_CONNECTOR_B3[22]"                             LOC = "M1";
NET   "RIGHT_CONNECTOR_B3[23]"                             LOC = "L4";
NET   "RIGHT_CONNECTOR_B3[24]"                             LOC = "L5";
NET   "RIGHT_CONNECTOR_B3[25]"                             LOC = "J2";
NET   "RIGHT_CONNECTOR_B3[26]"                             LOC = "K2";
NET   "RIGHT_CONNECTOR_B3[27]"                             LOC = "J6";
NET   "RIGHT_CONNECTOR_B3[28]"                             LOC = "K6";
NET   "RIGHT_CONNECTOR_B3[29]"                             LOC = "G2";
NET   "RIGHT_CONNECTOR_B3[30]"                             LOC = "H2";
NET   "RIGHT_CONNECTOR_B4[32]"                             LOC = "G4";
NET   "RIGHT_CONNECTOR_B4[33]"                             LOC = "H4";
NET   "RIGHT_CONNECTOR_B4[34]"                             LOC = "F1";
NET   "RIGHT_CONNECTOR_B4[35]"                             LOC = "G1";
NET   "RIGHT_CONNECTOR_B4[36]"                             LOC = "D1";
NET   "RIGHT_CONNECTOR_B4[37]"                             LOC = "E1";
NET   "RIGHT_CONNECTOR_B4[38]"                             LOC = "A1";
NET   "RIGHT_CONNECTOR_B4[39]"                             LOC = "B1";

NET   "RIGHT_CONNECTOR_A[1]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[2]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[3]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[4]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[5]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[6]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[7]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[8]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[9]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[10]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[11]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[12]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[13]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[14]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[15]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[16]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[17]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[18]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[19]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[20]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[21]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[22]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[23]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[24]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[25]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[26]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[27]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[28]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[29]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[30]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[31]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[32]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[33]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[34]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[35]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[36]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[37]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_A[38]" IOSTANDARD = LVCMOS33;

NET   "RIGHT_CONNECTOR_B1[1]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B1[2]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B1[3]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B1[4]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[6]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[7]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[8]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[9]"  IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[10]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[11]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[12]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[13]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[14]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[15]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[16]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[17]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[18]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B2[19]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[21]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[22]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[23]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[24]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[25]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[26]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[27]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[28]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[29]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B3[30]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[32]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[33]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[34]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[35]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[36]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[37]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[38]" IOSTANDARD = LVCMOS33;
NET   "RIGHT_CONNECTOR_B4[39]" IOSTANDARD = LVCMOS33;

#----------------------------------------------------------------
# LEFT CONNECTOR
#----------------------------------------------------------------

NET   "LEFT_CONNECTOR_A[1]"                             LOC = "AB1";
NET   "LEFT_CONNECTOR_A[2]"                             LOC = "AA1";
NET   "LEFT_CONNECTOR_A[3]"                             LOC = "AA3";
NET   "LEFT_CONNECTOR_A[4]"                             LOC = "Y3";
NET   "LEFT_CONNECTOR_A[5]"                             LOC = "AB5";
NET   "LEFT_CONNECTOR_A[6]"                             LOC = "AA5";
NET   "LEFT_CONNECTOR_A[7]"                             LOC = "AA6";
NET   "LEFT_CONNECTOR_A[8]"                             LOC = "Y6";
NET   "LEFT_CONNECTOR_A[9]"                             LOC = "AB8";
NET   "LEFT_CONNECTOR_A[10]"                             LOC = "AA8";
NET   "LEFT_CONNECTOR_A[11]"                             LOC = "Y9";
NET   "LEFT_CONNECTOR_A[12]"                             LOC = "W9";
NET   "LEFT_CONNECTOR_A[13]"                             LOC = "AB12";
NET   "LEFT_CONNECTOR_A[14]"                             LOC = "AB11";
NET   "LEFT_CONNECTOR_A[15]"                             LOC = "AB13";
NET   "LEFT_CONNECTOR_A[16]"                             LOC = "AA13";
NET   "LEFT_CONNECTOR_A[17]"                             LOC = "AB15";
NET   "LEFT_CONNECTOR_A[18]"                             LOC = "AA15";
NET   "LEFT_CONNECTOR_A[19]"                             LOC = "AB13";
NET   "LEFT_CONNECTOR_A[20]"                             LOC = "AA13";
NET   "LEFT_CONNECTOR_A[21]"                             LOC = "AB17";
NET   "LEFT_CONNECTOR_A[22]"                             LOC = "AB16";
NET   "LEFT_CONNECTOR_A[23]"                             LOC = "AA14";
NET   "LEFT_CONNECTOR_A[24]"                             LOC = "Y13";
NET   "LEFT_CONNECTOR_A[25]"                             LOC = "W16";
NET   "LEFT_CONNECTOR_A[26]"                             LOC = "W15";
NET   "LEFT_CONNECTOR_A[27]"                             LOC = "U16";
NET   "LEFT_CONNECTOR_A[28]"                             LOC = "T16";
NET   "LEFT_CONNECTOR_A[29]"                             LOC = "AB12";
NET   "LEFT_CONNECTOR_A[30]"                             LOC = "AB11";
NET   "LEFT_CONNECTOR_A[31]"                             LOC = "W14";

NET   "LEFT_CONNECTOR_B1[1]"                             LOC = "AB2";
NET   "LEFT_CONNECTOR_B1[2]"                             LOC = "AB3";
NET   "LEFT_CONNECTOR_B1[3]"                             LOC = "AA4";
NET   "LEFT_CONNECTOR_B1[4]"                             LOC = "Y4";
NET   "LEFT_CONNECTOR_B2[6]"                             LOC = "AB6";
NET   "LEFT_CONNECTOR_B2[7]"                             LOC = "AB7";
NET   "LEFT_CONNECTOR_B2[8]"                             LOC = "W5";
NET   "LEFT_CONNECTOR_B2[9]"                             LOC = "W6";
NET   "LEFT_CONNECTOR_B2[10]"                             LOC = "Y7";
NET   "LEFT_CONNECTOR_B2[11]"                             LOC = "Y8";
NET   "LEFT_CONNECTOR_B2[12]"                             LOC = "AB10";
NET   "LEFT_CONNECTOR_B2[13]"                             LOC = "AA9";
NET   "LEFT_CONNECTOR_B2[14]"                             LOC = "AA11";
NET   "LEFT_CONNECTOR_B2[15]"                             LOC = "AA10";
NET   "LEFT_CONNECTOR_B2[16]"                             LOC = "Y14";

NET   "LEFT_CONNECTOR_A[1]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[2]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[3]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[4]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[5]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[6]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[7]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[8]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[9]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[10]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[11]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[12]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[13]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[14]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[15]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[16]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[17]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[18]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[19]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[20]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[21]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[22]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[23]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[24]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[25]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[26]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[27]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[28]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[29]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[30]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_A[31]" IOSTANDARD = LVCMOS33;

NET   "LEFT_CONNECTOR_B1[1]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B1[2]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B1[3]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B1[4]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[6]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[7]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[8]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[9]"  IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[10]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[11]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[12]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[13]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[14]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[15]" IOSTANDARD = LVCMOS33;
NET   "LEFT_CONNECTOR_B2[16]" IOSTANDARD = LVCMOS33;
